{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":5,"n_cols":9,"rows_kept":5,"flags":["formulas_cached_only"]}
["序号","设备名称","品牌","型号","参数","单位","单价限价","数量","总价"]
[1,"床头呼叫器","来邦",null,"功能参数：纤薄机身，含手持，壁挂式安装在设备带上。\n功能简介：\n呼叫/解除：支持呼叫护士站主机与解除呼叫。\n双工对讲：支持与护士站主机全双工对讲。\n对讲方式：采用回音消除技术，支持全双工对讲，对讲音频采样率不低于16KHz。\n护理代接：在门口机进入护理状态下，通过床位分机接听其他病房分机呼叫，并双向对讲。\n接口多样：支持外接输液报警器、防水按钮、门灯。\n在线升级：支持在线升级软件。\n供电方式：三芯总线制供电。","台",280,70]
[2,"信号线","扬丰","RVV3*1.5","铜芯聚氯乙烯绝缘聚氯乙烯护套软线","米",6,1050]
[3,"安装调试",{"$nulls":3},"项",10500,1]
[4,"合计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}